# Insertable entrance aid EH S

# **Insertable entrance aid,** with design certification in accordance with DIN 19572, made of 1.4307 (AISI 304 L) stainless steel, for safety access ladders with 300 mm, 400 mm, 500 mm width.

Overall length: 1200 mm.

Entrance aid in accordance with DIN 19572.

Access ladders must have a handhold at their exit. This requirement is deemed to be fulfilled if one or both handles of a ladder project at least 1.1m beyond the exit height.

Ladder width = mm.

The insertable entrance aid has hooks welded on so that it can be hung onto the top rung and remain   
inside the manhole.

Completely shielded arc welded, acid-treated in a pickling bath and passivated.

**Options:**

➤ 1.4404 (AISI 316 L) stainless steel